Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# tunnel mpls affinity

#### Syntax

tunnel mpls [ traffic-eng ] affinity affinity [ mask mask ]

no tunnel mpls [ traffic-eng ] affinity

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Assigns an affinity to the tunnel that specifies the class of resources—resource attributes—associated with the tunnel. The no version removes the affinity from the tunnel.

#### Options

- traffic-eng—Specifies optional keyword for compatibility with non–E Series implementations
- affinity—Attributes that must be configured on the interface in order to be considered by the tunnel; in the range 0x0–0xFFFFFFFF; default value is 0x0
- mask—Mask to identify attributes to be checked and therefore the attribute flags that a link (interface) must have in order to be used by a tunnel: a 1 signifies that the attribute value must match the tunnel’s corresponding affinity bit; a 0 signifies that the attribute value does not matter and does not have to match the tunnel’s affinity bit; in the range 0x0–0xFFFFFFFF; default value is 0x0000FFFF

#### Mode

Interface Configuration, Tunnel Profile Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out