Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Creating or Modifying Classifier Control Lists for VLAN Policy Lists

# vlan classifier-list

#### Syntax

vlan classifier-list classifierName
[ traffic-class className ] [ color { green | yellow | red } ]
[ user-packet-class userPacketClassValue ] [ user-priority userPriorityValue ]

no vlan classifier-list classifierName [ classifierNumber ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Creates or modifies a VLAN classifier control list. The no version deletes the classifier control list.

#### Options

- classifierName—Name of a classifier list entry
- className—Name of a traffic class; the router supports up to eight traffic classes
- green—Matches packet color to green, indicating a low drop preference
- yellow—Matches packet color to yellow, indicating a medium drop preference
- red—Matches packet color to red, indicating a high drop preference
- userPacketClassValue—Value of the user packet class in the range 0–15
- userPriorityValue—Value of the user priority bits in the range 0–7
- classifierNumber—Index of the classifier control list entry to be deleted; an integer in the range 1–10000

#### Mode

Global Configuration

## Related Documentation

- Creating or Modifying Classifier Control Lists for VLAN Policy Lists

#### Published: 2010-10-19

Help
|
My Account
|
Log Out