Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# profile vlan bulk-config

#### Syntax

profile vlan bulk-config bulkConfigName profileName

no profile vlan bulk-config bulkConfigName

#### Release Information

Command introduced in JunosE Release 7.3.0.

#### Description

Assigns the base profile configured for a dynamic VLAN subinterface to the VLAN range configured on a static VLAN major interface with the vlan bulk-config command. The no version removes the base profile assignment.

#### Options

- bulkConfigName—Name of the VLAN range; string of up to 80 characters
- profileName—Profile name of up to 80 characters

#### Mode

Interface Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out