Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Configuring a Parameter Definition to Shape Ethernet Traffic Using Cell Mode
- Example: QoS Parameter Configuration for QoS Cell Mode and Byte Adjustment for Cell Shaping
- For more information about configuring scheduler rates for QoS parameters, see Scheduler Profiles and Parameter Expressions for QoS Administrators
- For more information about the QoS downstream rate application, see QoS Downstream Rate Application Overview
- controlled-interface-type
- instance-interface-type
- interface gigabitEthernet
- ip address
- qos-parameter
- qos-parameter-define
- scheduler-profile
- svlan qos-parameter
- traffic-class
- vlan id

# Configuring a Parameter Definition to Shape Ethernet Traffic Using Cell Mode

To associate a parameter instance with the QoS cell mode application:

1. Configure traffic classes.
   host1(config)#traffic-class voice host1(config-traffic-class)#exit host1(config)#traffic-class best-effort host1(config-traffic-class)#exit
2. Create a parameter definition.
   1. Configure the QoS parameter name and the application.
      host1(config)#qos-parameter-define shaping-mode application qos-cell-mode
   2. Configure a controlled-interface type.
      host1(config-qos-parameter-define)#controlled-interface-type vlan host1(config-qos-parameter-define)#controlled-interface-type ip
   3. Configure an instance-interface type.
      host1(config-qos-parameter-define)#instance-interface-type vlan
3. Create the parameter instance and configure the shaping mode.

   When you create the parameter instance and configure the shaping mode, the value of frame shaping mode is 0; the value for cell shaping mode is 1.

   host1(config)#interface gigabitEthernet 6/0/2 host1(config-if)#encapsulation vlan host1(config-if)#interface gigabitEthernet 6/0/2.1 host1(config-if)#vlan id 1 host1(config-if)#qos-parameter cell-mode 1 host1(config-if)#ip address 6.10.10.10 255.255.255.255 host1(config-if)#exit host1(config)#interface gigabitEthernet 6/0/2 host1(config-if)#svlan 1 qos-parameter cell-mode 1 host1(config-if)#exit host1(config)#interface gigabitEthernet 6/0/2 host1(config-if)#qos-parameter cell-mode 1

## Related Documentation

- Configuring a Parameter Definition to Shape Ethernet Traffic Using Cell Mode
- Example: QoS Parameter Configuration for QoS Cell Mode and Byte Adjustment for Cell Shaping
- For more information about configuring scheduler rates for QoS parameters, see Scheduler Profiles and Parameter Expressions for QoS Administrators
- For more information about the QoS downstream rate application, see QoS Downstream Rate Application Overview
- controlled-interface-type
- instance-interface-type
- interface gigabitEthernet
- ip address
- qos-parameter
- qos-parameter-define
- scheduler-profile
- svlan qos-parameter
- traffic-class
- vlan id

#### Published: 2010-10-04

Help
|
My Account
|
Log Out