Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- show ip http server

# Monitoring the Configuration of the HTTP Local Server

#### Purpose

Display information about the configuration of the HTTP local server.

#### Action

To display information about the HTTP local server:

    host1#show ip http server
      Admin status: enabled
      Access class: not defined
      Listening port: 80
      Same host limit: 3
      Protocol: IPv6

#### Meaning

Table 1 lists the show ip http server command output fields.

Table 1: show ip http server Output Fields

Field Name | Field Description
--- | ---
Admin status | Status of the HTTP local server in the software: enabled or disabled. Enabled implies that the HTTP local server can listen for IPv4 , IPv6, or both IPv4 and IPv6 exception packets.
Access class | Name of a standard IP access list that determines which hosts can log on to the HTTP local server
Listening port | Port that the HTTP local server uses to track requests for connection
Same host limit | Maximum number of connections allowed between one IP address and the HTTP local server
Protocol | Protocols that the HTTP local server is listening for: IPv4, IPv6, or IPv4 and IPv6.

## Related Documentation

- show ip http server

#### Published: 2010-10-12

Help
|
My Account
|
Log Out