Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Configuring Simple Shared Shaper Algorithm Variables

# reaction-factor

#### Syntax

reaction-factor reactionFactor

no reaction-factor

#### Release Information

Command introduced in JunosE Release 8.0.0.

#### Description

Specifies the reaction factor for all simple shared shapers on the router. The reaction factor determines how the shared shaper reacts to changes in the measured rate. The no version removes the specified reaction factor from all simple shared shapers on the router.

#### Options

- reaction-factor—Percentage in the range 0–1000; default value is 200

#### Mode

QoS Shared Shaper Control Configuration

## Related Documentation

- Configuring Simple Shared Shaper Algorithm Variables

#### Published: 2010-10-19

Help
|
My Account
|
Log Out