Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# redundancy revertive

#### Syntax

[ no ] redundancy revertive [ timeOfDay ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables the router to revert from spare line modules to available primary line modules automatically. The no version reverts to the default situation, in which there is no automatic reversion from spare to primary line modules.

#### Options

- timeOfDay—Time, in 24-hour format (00:00:00), at which the router reverts to the available primary line modules every day

#### Mode

Global Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out