Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# ppp reassembly

#### Syntax

ppp reassembly [ mrru ]

no ppp reassembly

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables reassembly on an MLPPP link interface and optionally specifies the administrative MRRU value, in octets, for the link. The no version disables reassembly on the link and restores the default value, which is the link’s local MRU.

#### Options

- mrru—Maximum allowable size of the PPP packet payload that the router can receive, in the range 64–65535; default value is the link’s local MRU

#### Mode

Interface Configuration, Profile Configuration, Subinterface Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out