# frame-relay lmi-n392dte

#### Syntax

frame-relay lmi-n392dte threshold

no frame-relay lmi-n392dte

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the error threshold counter (N392) on a DTE interface. The no version removes current setting and sets the default.

#### Options

- threshold—Positive number in the range 1–10; number of errors that will place the interface in an operationally down state; default value is 3 errors

#### Mode

Interface Configuration