# ip igmp promiscuous

#### Syntax

ip igmp promiscuous { on | off }

no ip igmp promiscuous

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables the specified interface to accept IGMP reports from hosts on any subnet. The no version specifies that an IGMP interface should use the Router Configuration mode setting (see the igmp promiscuous command) to determine from which subnets it can accept IGMP reports.

#### Options

- on—Enables the interface to accept IGMP reports from hosts on any subnet
- off—Allows the interface to accept IGMP reports only from hosts on subnets associated with this interface

#### Mode

Interface Configuration, Profile Configuration