Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# redundancy revert

#### Syntax

[ no ] redundancy revert slotNumber
[ startTime [ [ startMonth startDay | startDay startMonth ] startYear ] ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Forces the router to revert to the primary line module in the specified slot. If you specify a time or time and date, reversion occurs when the primary line module becomes available after that time. Otherwise, reversion occurs immediately. Issuing this command causes reversion once; after reboot, the router returns to the settings configured in the software. The no version has no effect.

#### Options

- slotNumber—Number of the slot in which the primary line module resides
- startTime—Time, in 24-hour format (00:00:00), at which the router reverts to this line module
- startMonth—Name of the month in which the router reverts to this line module
- startDay—Day of the month on which the router reverts to this line module
- startYear—Four-digit year in which the router reverts to this line module

#### Mode

Privileged Exec

#### Published: 2010-10-19

Help
|
My Account
|
Log Out