Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# oam cc

#### Syntax

oam cc [ segment | end-to-end ] { source | sink | both }

no oam cc

#### Release Information

Command introduced in JunosE Release 7.1.0.
ATM VC Class Configuration mode added in JunosE Release 7.3.0.

#### Description

In ATM VC Configuration mode, enables F5 OAM continuity check (CC) verification on an ATM PVC. The oam cc command is valid only for data PVCs; you cannot use this command for control (ILMI or signaling) PVCs. The no version restores the default behavior, which disables F5 OAM CC verification and restores the default setting for cell termination, end-to-end.

In ATM VC Class Configuration mode, enables F5 OAM CC verification as part of a VC class definition that you assign to an ATM data PVC. The no version restores the default setting for cell termination, end-to-end, in the VC class.

#### Options

- segment—Opens an F5 OAM CC segment cell flow
- end-to-end—Opens an F5 OAM CC end-to-end cell flow
- source—Enables this VC as the source point (cell generator)
- sink—Enables this VC as a sink point (cell receiver)
- both—Enables this VC as both a sink point and a source point

#### Mode

ATM VC Configuration, ATM VC Class Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out