# ip igmp static-include

#### Syntax

[ no ] ip igmp static-include sourceAddress groupAddress

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Assigns an interface to handle multicast traffic for one or more (S,G) combinations. The no version removes the (S,G) association from the interface.

#### Options

- sourceAddress—Address of the source
- groupAddress—Address of the group

#### Mode

Interface Configuration, Profile Configuration