Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# show resource

#### Syntax

show resource [ [ if-type { atm-active-sub-if | atm-sub-if | atm-vc | ip | ppp-link }
[ system | slot slot ] ] | [ threshold [ trap [ status ] ] ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays statistical information about resources and their current threshold configurations.

#### Options

- if-type—Indicates interface type; see Interface Types and Specifiers
- atm-active-sub-if—Active ATM subinterfaces
- atm-sub-if—Both active and inactive ATM subinterfaces
- atm-vc—ATM virtual circuits
- ip—IP interfaces
- ppp-link—PPP link interfaces
- system—All slots on the system
- slot—Number of the chassis slot in the range 0–2 (ERX310 model), 0–6 (ERX7xx models), and 0–13 (ERX14xx models)
- threshold—Displays threshold information (optional keyword when used alone)
- trap—Displays threshold trap status
- status—Displays threshold trap status (optional keyword)

#### Mode

Privileged Exec

#### Published: 2010-10-19

Help
|
My Account
|
Log Out