# debug ipv6 ospf

#### Syntax

debug ipv6 ospf ospfLog [ severity { severityValue | severityNumber } ]
[ verbosity verbosityLevel ]

no debug ipv6 ospf ospfLog

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Shows information about the selected variable. The no version disables the display.

#### Options

- ospfLog—OSPF log of interest; one of the following options:
  - adj—OSPF adjacency events
  - elect-dr—OSPF designated router election
  - events—OSPF general events
  - lsa—OSPF link-state advertisements events
  - neighbor—OSPF neighbor state machine
  - packets-rcvd—OSPF packets received
  - packets-sent—OSPF packets sent
  - route—OSPF route events
  - spf—All OSPF shortest path first calculation events
  - spf-ext—OSPF shortest path first external route calculation events
  - spf-inter—OSPF shortest path first interarea route calculation events
  - spf-intra—OSPF shortest path first intra-area route calculation events
- severity—Specifies the minimum severity of the log messages displayed for the selected category; described either by a descriptive term—severityValue—or by a corresponding number—severityNumber—in the range 0–7; the lower the number, the higher the priority:
  - emergency or 0—System unusable
  - alert or 1—Immediate action needed
  - critical or 2—Critical condition exists
  - error or 3—Error condition
  - warning or 4—Warning condition
  - notice or 5—Normal but significant condition
  - info or 6—Informational message
  - debug or 7—Debug message
- verbosityLevel—Verbosity of the log category's messages; can be any of the following:
  - low—Terse
  - medium—Moderate detail
  - high—Verbose

#### Mode

Privileged Exec