# trigger delay

#### Syntax

trigger delay msec delayTime

no trigger delay

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the time duration used to determine when a SONET/SDH defect at the line or section layer becomes an alarm. The no version restores the default setting, 2500 milliseconds.

#### Options

- delayTime—Time in the range 0–2500 milliseconds

#### Mode

Controller Configuration