Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Configuring a QoS Profile
- Attaching a QoS Profile to an Interface
- Configuring Shadow Nodes
- Configuring a Basic Parameter Definition for QoS Administrators
- Creating Parameter Instances
- Attaching a QoS Profile to an Interface Superset or an Interface Set
- Creating a QoS Parameter on an Interface Superset or Interface Set

# qos-profile

#### Syntax

[ no ] qos-profile qosProfileName

#### Release Information

Command introduced before JunosE Release 7.1.0.
Profile Configuration mode added in JunosE Release 7.2.0.

QoS Interface Set Configuration and QoS Interface Superset Configuration modes added in JunosE Release 9.2.0.

#### Description

In Global Configuration mode, creates a QoS profile on the router and enters QoS Profile Configuration mode. The no version deletes the QoS profile.

In Interface Configuration mode, attaches a QoS profile to an interface. The no version detaches the QoS profile from the interface.

In Profile Configuration mode, adds a QoS profile command for use with Service Manager. When the service is activated, the QoS profile is created and attached to the subscriber interface. The no version removes the QoS profile from the profile.

In QoS Interface Set Configuration mode, attaches a QoS profile to the QoS interface set. The no version detaches the QoS profile from the interface set.

In QoS Interface Superset Configuration mode, attaches a QoS profile to the QoS interface superset. The no version detaches the QoS profile from the interface superset.

#### Options

- qosProfileName—Name of the QoS profile

#### Mode

Global Configuration, Interface Configuration, Profile Configuration, QoS Interface Set Configuration, QoS Interface Superset Configuration

## Related Documentation

- Configuring a QoS Profile
- Attaching a QoS Profile to an Interface
- Configuring Shadow Nodes
- Configuring a Basic Parameter Definition for QoS Administrators
- Creating Parameter Instances
- Attaching a QoS Profile to an Interface Superset or an Interface Set
- Creating a QoS Parameter on an Interface Superset or Interface Set

#### Published: 2010-10-19

Help
|
My Account
|
Log Out