# diag-level

#### Syntax

diag-level [ normal ] [ bypass ]

#### Release Information

Command introduced in JunosE Release 9.2.0.

#### Description

Sets the diagnostics level on the active or standby SRP module to reduce boot time during a cold and a warm boot. The default diagnostics level is normal. There is no no version.

#### Options

- normal—executes full diagnostics on the boot of the line card

  bypass—skips diagnostic tests on the boot of the line card

#### Mode

Global Configuration