Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# show redundancy line-card

#### Syntax

show redundancy line-card [ slot slotNum ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

slot keyword and slotNum variable added in JunosE Release 11.3.0.

#### Description

Displays redundancy information specific to line modules, including supported redundancy modes and high availability status for a line module installed in a particular slot. If you enter this command without the slot keyword, redundancy details for all line modules on a router are displayed.

#### Options

- slotNum—Number of the slot in which the line module resides in the router; for the E120 router, a number in the range 0–5; for the E320 router, a number in the range 0–5 or 11–16
- filter—See Filtering show Commands

#### Mode

Privileged Exec

#### Published: 2010-10-19

Help
|
My Account
|
Log Out