# ip dvmrp route-hog-notification

#### Syntax

[ no ] ip dvmrp route-hog-notification [ limit ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the number of DVMRP routes that the router can record before it generates a system log warning message. The no version restores the default setting, 10,000 routes.

#### Options

- limit—Number in the range 0–2147483647

#### Mode

Global Configuration