Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Monitoring the Configuration of QoS Profiles

# show qos-profile

#### Syntax

To display information about all QoS profiles or a specific QoS profile:

show qos-profile [ qosProfileName ] [ brief ] [ filter ]

To display information about the QoS profiles attached to a specific interface:

show qos-profile references interface interfaceType interfaceSpecifier
[ atmVpi | s-vlanIdValue ] [ explicit ] [ brief ] [ filter ]

To display information about the QoS profiles attached to a specific L2TP session:

show qos-profile references lt2p session sessionName [ explicit ] [ brief ] [ filter ]

To display information about the QoS profiles attached to a specific tunnel-service interface:

show qos-profile references tunnel-server interfaceType [ explicit ] [ brief ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
references keyword added in JunosE Release 7.1.0.

#### Description

Displays information about QoS profiles configured on the router. Use the references keyword to display information about QoS profiles attached to an interface, L2TP session, or tunnel-service interface.

#### Options

- qosProfileName—Name of the QoS profile
- references—Displays interface profiles that reference this profile
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- atmVpi—Virtual path identifier of this PVC; number in the range 0–255
- s-vlanIdValue—S-VLAN ID number in the range 0–4095
- sessionName —Name of the L2TP session
- explicit—Displays attachments for QoS profiles only on the specified interface and not QoS profiles stacked above the interface
- brief—Displays information in a condensed format
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

## Related Documentation

- Monitoring the Configuration of QoS Profiles

#### Published: 2010-10-19

Help
|
My Account
|
Log Out