Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Chapter 17, Configuring Dynamic Interfaces
- ppp multilink multiclass traffic-class

# Configuring Traffic Classes on Multiclass MLPPP Interfaces

You can configure mapping of QoS traffic classes to multilink classes. The best-effort QoS traffic class is mapped to multilink class 0 by default.

To configure mapping of QoS traffic classes to multilink classes:

- Specify the QoS traffic classes to be mapped to the multilink classes.

  - To map QoS traffic classes to multilink classes in a dynamic profile:

    host1(config-profile)#ppp multilink multiclass traffic-class best-effort voice otherData video

  - To map QoS traffic classes to multilink classes in a static MLPPP interface:

    host1(config-if)#ppp multilink multiclass traffic-class best-effort voice otherData video

  | Note: You must include the best-effort traffic class in the ppp multilink multiclass traffic-class command, or the command fails.

## Related Documentation

- Chapter 17, Configuring Dynamic Interfaces
- ppp multilink multiclass traffic-class

#### Published: 2010-10-13

Help
|
My Account
|
Log Out