# ipv6 ospf network

#### Syntax

ipv6 ospf [ processId ] network { broadcast | point-to-point }

no ipv6 ospf [ processId ] network

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies a network type (broadcast or point-to-point) for an interface. The no version resets the path cost to the default.

#### Options

- processId—Integer in the range 1–65535

#### Mode

Interface Configuration, Subinterface Configuration