Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- See Monitoring MPLS Layer 2 Interfaces for Layer 2 Services over MPLS in JunosE BGP and MPLS Configuration Guide
- Monitoring the Policy Configuration of Layer 2 Services over MPLS

# show mpls l2transport interface

#### Syntax

show mpls l2transport interface
[ summary | [ interfaceType interfaceSpecifier ] [ brief | detail ] [ state not-up ] [ delta ] ]
[ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
summary keyword added in JunosE Release 8.0.0.

#### Description

Displays status and configuration information about layer 2 services over MPLS (also known as Martini, or layer 2 transport) on the router or on specific interfaces.

#### Options

- summary—Displays summary information about layer 2 services over MPLS
- interfaceType—Displays information only for the specified MPLS interface; if not specified, information for all interfaces is displayed
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- brief—Displays limited interface information
- detail—Provides expanded information about layer 2 services, rather than a summary
- state not-up—Displays information only about interfaces that are not up
- delta—Displays baselined statistics
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

## Related Documentation

- See Monitoring MPLS Layer 2 Interfaces for Layer 2 Services over MPLS in JunosE BGP and MPLS Configuration Guide
- Monitoring the Policy Configuration of Layer 2 Services over MPLS

#### Published: 2010-10-19

Help
|
My Account
|
Log Out