Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# neighbor ibgp-singlehop

#### Syntax

[ no | default ] neighbor { ipAddress | ipv6Address | peerGroupName } ibgp-singlehop

#### Release Information

Command introduced in JunosE Release 8.0.0.

#### Description

Configures an internal BGP peer to be a single-hop (non-multihop) peer. The no version restores the default, wherein internal peer cannot be a single hop. The default version removes the explicit configuration from the peer or peer group and reestablishes inheritance of the feature configuration.

#### Options

- ipAddress—IP address of BGP neighbor
- ipv6Address—IPv6 address of BGP neighbor
- peerGroupName—Name of a BGP peer group. If you specify a BGP peer group by using the peerGroupName argument, all the members of the peer group inherit the characteristic configured with this command, unless it is overridden for a specific peer.

#### Mode

Address Family Configuration, Router Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out