Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# slot ignore-diagnostic-failure

#### Syntax

[ no ] slot ignore-diagnostic-failure slotNum

#### Release Information

Command introduced in JunosE Release 9.3.0.

#### Description

Enables you to ignore diagnostics test failures on the line module or SRP. The no version returns you to the default allowing diagnostic test failures to occur.

#### Options

- slotNum—Number of the selected slot in the router; for ERX7xx models, a number in the range 0–6; for ERX14xx models, a number in the range 0–13; for the ERX310 router, a number in the range 1–2; for the E120 router, a number in the range 0–5; for the E320 router, a number in the range 0–16

#### Mode

Global Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out