Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# transform

#### Syntax

transform transform0
[ transform1 [ transform2 [ transform3 [ transform4 [ transform5 ] ] ] ] ]

no transform

#### Release Information

Command introduced in JunosE Release 7.3.0.

#### Description

Specifies the eligible transforms for this profile for IPSec source address negotiations. You can specify up to six transform algorithms for this profile. The no version resets the transform to the default, esp-3des-sha1.

#### Options

- transform0 through transform5—AH or ESP transform

#### Mode

IPSec Tunnel Profile Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out