# show mpls tunnels

#### Syntax

show mpls [ traffic-eng ] tunnels [ name tunnelName ]
[ role { all | head | tail | middle | remote } | up | down ]
[ source-id sourceAddress [ srcId ] ] [ destination destAddr ]
[ interface interfaceType interfaceSpecifier ] [ brief | count-only ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays status and configuration for all tunnels or for a specific tunnel in the current router context.

#### Options

- traffic-eng—Specifies optional keyword for compatibility with non–E Series implementations
- tunnelName—Name of tunnel or minor interface to be displayed
- role—Displays tunnels in which the router has a specified role:
  - all—Displays all tunnels of which the router is a part
  - head—Displays tunnels where the router is the ingress router, or tunnel headend
  - tail—Displays tunnels where router is the egress router, or tunnel tailend (endpoint or destination of the tunnel)
  - middle—Displays tunnels where router is a transit router on the tunnel
  - remote—Displays tunnels where router is a transit router or egress router (tailend)
- up—Displays tunnels that are up
- down—Displays tunnels that are down
- sourceAddress—Source address of tunnels to be displayed
- srcId—Local ID associated with source address of tunnels to be displayed, an integer in the range 0–65535
- destAddress—Destination address of tunnels to be displayed
- interface—Displays information for the specified interface
  - interfaceType—Interface type; see Interface Types and Specifiers
  - interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- brief—Displays only brief or summary information about the tunnels
- count-only—Displays a count for entries that match the specified conditions
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec