# Clearing the Redundancy History

To clear the stateful SRP switchover history for the router:

- Issue the clear redundancy history command:
  host1#clear redundancy history

There is no no version.

#### Related Documentation

- Monitoring the Redundancy History
- Monitoring the Redundancy Switchover History
- clear redundancy history
- show redundancy history
- show redundancy switchover-history