# nas-port-type ethernet

#### Syntax

nas-port-type ethernet { cable | wireless-80211 | wireless-cdma | wireless-umts |
wireless-1x-ev | wireless-other | iapp | value }

no nas-port-type ethernet

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the RADIUS NAS-Port-Type attribute (61) used for Ethernet interfaces. The no version removes the NAS-Port-Type setting.

#### Options

- cable—Cable
- wireless-80211—Wireless 802.11
- wireless-cdma—Wireless code division multiple access (CDMA)
- wireless-umts—Wireless universal mobile telecommunications system (UMTS)
- wireless-1x-ev—Wireless 1xEV
- wireless-other—Wireless other
- iapp—Inter Access Point Protocol (IAPP)
- value—Number in the range 0–65535

#### Mode

AAA Profile Configuration