Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# set metric

#### Syntax

set metric [ +relValue | -relValue | absValue ]

no set metric

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Modifies the metric value (for BGP, the MED) for a route that matches the route map by applying a relative or absolute metric. The no version removes the set clause from a route map.

| Note: You cannot have an absolute and a relative metric within the same route map sequence. Issuing either command overrides any previously configured metric in the route map.

#### Options

- +—Specifies that the value is added to the metric for routes matching the route map; immediately precedes the metric value with no intervening space
- –—Specifies that the value is subtracted from the metric for routes matching the route map; immediately precedes the metric value with no intervening space
- relValue—Number, in the range 0–4294967295
- absValue—Number, in the range 0–4294967295

#### Mode

Route Map Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out