Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- To add members to the interface superset, see Configuring Interface Sets for QoS
- Monitoring the Configuration of QoS Interface Supersets
- qos-interface-superset
- qos-interface-parent
- restricted

# Configuring Interface Supersets for QoS

Tasks to configure an interface superset for QoS include:

## Configuring an Interface Superset

To configure an interface superset that contains interface sets and logical interfaces:

1. Create the interface superset.
   host1(config)#qos-interface-super-set vlan-superset-shaping
2. Specify the parent interface for the superset.
   host1(config-interface-superset)#qos-interface-parent interface tenGigabitEthernet 4/0/0

   You can configure an Ethernet major interface, an ATM major interface, or a LAG for the parent interface. You must define the parent before you add interface sets or subinterfaces to the interface superset.

## Restricting an Interface Superset to an S-VLAN ID or an ATM VP

When you configure interface supersets for VLANs or ATM VCs, the member interfaces normally span different S-VLAN IDs or ATM VPs.

Optionally, you can restrict all interface members of a VLAN superset to a specific S-VLAN ID, or all members of an ATM VC to a specific ATM VP.

To restrict the interface members of an interface superset:

1. Specify the interface superset.
   host1(config)qos-interface-superset residential-customers
2. Restrict the interfaces in the interface superset.

   For VLAN supersets, restrict the VLAN subinterfaces to an S-VLAN ID:

   host1(config-qos-interface-superset)#restricted interface tenGigabitEthernet 4/0/0 svlan id 2

   For ATM VC supersets, restrict an ATM VC to an ATM VP:

   host1(config-qos-interface-superset)#restricted interface atm 2/0/0 atm-vp 2

## Related Documentation

- To add members to the interface superset, see Configuring Interface Sets for QoS
- Monitoring the Configuration of QoS Interface Supersets
- qos-interface-superset
- qos-interface-parent
- restricted

#### Published: 2010-09-22

Help
|
My Account
|
Log Out