Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Supported Interface Types for QoS Profiles
- Configuring a QoS Profile
- Configuring Shadow Nodes

# Supported Interface Types for QoS Profiles

Each QoS profile command begins with a keyword that designates an interface type.

Table 1 lists the interface types and the commands that you can use with them.

Table 1: Interface Types and Supported Commands

Interface Type | Queue | Node | Group | Shadow Node
--- | --- | --- | --- | ---
atm | ✓ | ✓ | ✓ | ✓
atm-vc | ✓ | ✓ | – | ✓
atm-vp | ✓ | ✓ | – | ✓
bridge | ✓ | ✓ | – | ✓
ethernet | ✓ | ✓ | ✓ | ✓
fr-vc | ✓ | ✓ | – | ✓
ip | ✓ | ✓ | – | ✓
ip-tunnel | ✓ | ✓ | – | ✓
ipv6 | ✓ | ✓ | – | ✓
l2tp-session | ✓ | ✓ | – | ✓
l2tp-tunnel | ✓ | ✓ | – | ✓
lsp | ✓ | ✓ | – | ✓
serial | ✓ | ✓ | ✓ | ✓
server-port | ✓ | ✓ | ✓ | ✓
svlan | ✓ | ✓ | – | ✓
vlan | ✓ | ✓ | – | ✓

## Related Documentation

- Supported Interface Types for QoS Profiles
- Configuring a QoS Profile
- Configuring Shadow Nodes

#### Published: 2010-09-22

Help
|
My Account
|
Log Out