# l2c max-branches

#### Syntax

[ no ] l2c max-branches maxBranches

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the maximum number of branches the ANCP end user can have. The no version returns the maximum number of branches to its default value (unlimited branches).

#### Options

- maxBranches—Maximum number of branches allowed for the ANCP end user in the range 1–64000

#### Mode

Interface Configuration, Subinterface Configuration