Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- show sscc info

# Monitoring SRC Client Connection Status

#### Purpose

Display the current status of the SRC client connection to the SAEs. The command output refers to the SRC client by its former name, SSC client.

#### Action

To display the status of the SRC client connection:

    host1#show sscc info
    The SSC Client configured protocols : IP(v4), DHCP(v4), L2TP(LAC)
    The SSC Client is currently unconnected
    The SSC Client configured servers are:
            Primary: 10.10.2.2:3
            Secondary: 0.0.0.0:0
            Tertiary: 0.0.0.0:0
            Local Source: FastEthernet 0/0, Local Source Address: 10.13.5.61
            The configured transport router is: default
            The configured retry timer is (seconds): 90
            The configured update-policy-request is: Enabled
            The connection state is: NoConnection
     SSC Client Statistics:
            Policy Commands received   0
            Policy Commands(List)      0
            Policy Commands(Acct)      0
            Bad Policy Cmds received   0
            Error Policy Cmds received 0
            Policy Reports sent        0
            Connection Open requests   0
            Connection Open completed  0
            Connection Closed sent     0
            Connection Closed remotely 0
            Create Interfaces sent     0
            Delete Interfaces sent     0
            Active IP Interfaces       2
            IP Interface Transitions   0
            Synchronizes received      0
            Synchronize Complete sent  0
            Internal Errors            0
            Communication Errors       0
            Tokens Seen                0
            Active Tokens              0
            Token Transitions          0
            Token Creates Sent         0
            Token Deletes Sent         0
            Active Addresses           0
            Address Transitions        0
            Create Addresses Sent      0
            Delete Addresses Sent      0
            Authentication Successes   0
            Authentication Failures    0

#### Meaning

Table 1 lists the show sscc info command output fields.

Table 1: show sscc info Output Fields

Field Name | Field Description
--- | ---
The SSC client configured protocols | Protocols that are enabled on the virtual router for policy and QoS management by the SRC software
The SSC client configured servers | IP addresses of the primary, secondary, and tertiary SAEs
Local Source | Fixed source interface for the TCP/COPS connection
Local Source Address | Fixed source address for the TCP/COPS connection
The configured transport router is | Router on which is TCP/COPS connection is established
The configured retry timer is (seconds) | Delay period the client waits for a response from the SAE before submitting request again
The configured update-policy-request is | Whether the router or the SRC client retrieves DSL line rate parameters, whenever the values change after connection establishment, from ANCP and transfers the details to the COPS server with other COPS messages, enabled or disabled
The connection state is | Current state of the TCP/COPS connection
SSC Client Statistics | Statistics about the connection between the SRC client and SAE Policy Commands received—Number of policy commands received on the SRC client connection Policy Commands(List)—Number of Policy Commands with subtype List Policy Commands(Acct)—Number of Policy Commands with subtype Accounting Bad Policy Cmds received—Number of Policy Commands received with bad policies Error Policy Cmds received—Number of Policy Commands received with errors Policy Reports sent—Number of Policy Reports sent Connection Open requests—Number of connections the SRC client has tried to open with a remote SAE Connection Open completed—Number of connections successfully open to the SAE Connection Closed sent—Number of connections the SRC client has closed Connection Closed remotely—Number of connections that were closed by the remote SAE Create Interfaces sent—Number of create interface indications sent to the SAE Delete Interfaces sent—Number of delete interface indications sent to the SAE Active IP Interfaces—Current number of active IP interfaces the SRC client is aware of IP Interface Transitions—Number of IP interface transitions logged by the SRC client Synchronizes received—Number of synchronization requests the SRC client received from the SAE Synchronize Complete sent—Number of synchronization complete indications sent Internal Errors—Number of internal errors Communication Errors—Number of errors with lower-layer communications (such as socket errors)

## Related Documentation

- show sscc info

#### Published: 2010-10-12

Help
|
My Account
|
Log Out