Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# write core

#### Syntax

write core [ standby-srp | slot slotNumber ] [ force ] [ reason reasonText ]

#### Release Information

Command introduced in JunosE Release 7.3.0.

#### Description

Reboots the active SRP module, the standby SRP module, or the module in a specified slot, and writes the core dump to a file. There is no no version.

#### Options

- standby-srp—Specifies the standby SRP module
- slotNumber—Number of a selected slot in the router; for ERX7xx models, a number in the range 0–6; for ERX14xx models, a number in the range 0–13; for the ERX310 router, a number in the range 0–2; for the E120 router, a number in the range 0–5; for the E320 router, a number in the range 0–16
- force—Prompts for confirmation to reboot when the router is in certain states, such as during the synchronization of SRP modules, that can lead to a loss of configuration data or an NVS corruption

  | Note: The force keyword is available when you specify a slot only if that slot is an SRP module slot.

- reasonText—Alphanumeric text string (1–255 characters long) that explains the request for a core dump and logs it in the reboot

#### Mode

Privileged Exec

#### Published: 2010-10-19

Help
|
My Account
|
Log Out