Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# pppoe profile

#### Syntax

[ no ] pppoe profile [ bridgedEthernet | ip | ppp | pppoe | any ] profileName

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Assigns a profile to a static PPPoE major interface. The profile configuration is used to dynamically configure an upper bridged Ethernet, IP, PPP, and/or PPPoE interface. The no version removes the profile assignment from the interface.

#### Options

- bridgedEthernet—Specifies a bridged Ethernet encapsulation type to which the profile applies
- ip—Specifies an IP encapsulation type to which the profile applies
- ppp—Specifies a PPP encapsulation type to which the profile applies
- pppoe—Specifies a PPPoE encapsulation type to which the profile applies
- any—Specifies any autoconfigured encapsulation that does not have a specific profile assignment
- profileName—Profile name of up to 80 characters

#### Mode

Interface Configuration, Subinterface Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out