# vlan profile

#### Syntax

[ no ] vlan profile upperInterfaceType profileName

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Adds a nested profile assignment to a base profile for a dynamic VLAN subinterface. A nested profile assignment references another profile that dynamically configures upper interface encapsulation types over the VLAN subinterface. The no version removes the profile assignment for the upper interface type.

#### Options

- upperInterfaceType—One of the following dynamic encapsulation types:
  - ip
  - pppoe
- profileName—Profile name of up to 80 characters

#### Mode

Profile Configuration