Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# ppp authentication

#### Syntax

ppp authentication [ virtual-router vrName ] { authProtocol }

no ppp authentication

#### Release Information

Command introduced before JunosE Release 7.1.0.
eap keyword added in JunosE Release 7.3.0.

#### Description

Requests authentication from a PPP peer router. The no version removes the authentication requirement.

#### Options

- vrName—Name of a virtual router to be used as the authentication virtual router
- authProtocol—One or more of the following protocols, in order of preference; if the peer router refuses to negotiate the first choice, then the local router requests the next specified protocol, and so on; if the peer router refuses to negotiate authentication, the local router terminates the session
  - eap—Specifies EAP authentication protocol
  - chap—Specifies CHAP authentication protocol
  - pap—Specifies PAP authentication protocol

#### Mode

Interface Configuration, Profile Configuration, Subinterface Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out