Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# show ipsec transport interface

#### Syntax

show ipsec transport interface [ detail ] [ application applicationType ]
[ state { up | down } ] [ interfaceName |
[ virtual-router vrName ] destination destAddress | local localAddress ] [ filter ]

To display summary information:

show ipsec transport interface summary

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays all details, including statistics, of IPSec transport connections that match the specified criteria.

#### Options

- detail—Includes statistics for the displayed connection
- applicationType—Application protected by IPSec transport connections
- state—Displays connections that are in the specified state, up or down
- interfaceName—Connection number that you want to display
- vrName—Name of a virtual router. If you do not specify a virtual router, the router displays connections on the current virtual router context. Notice that the local and destination IP addresses exist in the current virtual router context.
- destAddress—IP address of remote endpoint
- localAddress—IP address of local endpoint
- filter—See Filtering show Commands
- summary—Displays a summary of all IPSec transport connections

#### Mode

Privileged Exec

#### Published: 2010-10-19

Help
|
My Account
|
Log Out