Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# neighbor ebgp-multihop

#### Syntax

[ no | default ] neighbor { ipAddress | ipv6Address | peerGroupName } ebgp-multihop
[ ttl ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
ipv6Address variable added in JunosE Release 8.0.0.

#### Description

Allows BGP to accept route updates from external peers residing on networks that are not directly connected. The no version halts accepting such routers. The default version removes the explicit configuration from the peer or peer group and reestablishes inheritance of the feature configuration.

#### Options

- ipAddress—IP address of BGP neighbor
- ipv6Address—IPv6 address of BGP neighbor
- peerGroupName—Name of a BGP peer group. If you specify a BGP peer group by using the peerGroupName argument, all the members of the peer group inherit the characteristic configured with this command, unless it is overridden for a specific peer.
- ttl—Maximum number of hops to the peer, in the range 1–255; default value is 255

#### Mode

Address Family Configuration, Router Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out