Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Configuring a Basic Parameter Definition for QoS Administrators

# subscriber-interface-type

#### Syntax

subscriber-interface-type subscriberInterfaceType

no subscriber-interface-type { subscriberInterfaceType | all }

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Assigns a subscriber-interface type to a QoS parameter definition. Subscriber-interface types represent subscriber interfaces to which QoS clients can apply QoS parameter instances obtained through RADIUS, SRC, or QoS profiles. You can specify up to four subscriber-interface types for each parameter definition. The no version removes the subscriber-interface type from the parameter definition.

#### Options

- subscriberInterfaceType—One of the following subscriber-interface types: atm-vc, ip, ipv6, l2tp-session, vlan
- all—Removes all subscriber-interface types

#### Mode

QoS Parameter Definition

## Related Documentation

- Configuring a Basic Parameter Definition for QoS Administrators

#### Published: 2010-10-19

Help
|
My Account
|
Log Out