# member-interface

#### Syntax

[ no ] member-interface interfaceType interfaceSpecifier

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Adds a member interface, also known as a bundle member, to an MLPPP bundle, an MLFR bundle, or an IEEE 802.3ad link aggregation group (LAG) bundle. The no version removes the specified member interface from the bundle.

#### Options

- interfaceType—One of the following interface types listed in Interface Types and Specifiers
  - serial (MLFR bundle or MLPPP bundle)
  - pos (MLFR bundle only)
  - fastEthernet (IEEE 802.3ad LAG bundle only)
  - gigabitEthernet (IEEE 802.3ad LAG bundle only)
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

Interface Configuration, Subinterface Configuration