# radius override nas-ip-addr tunnel-client-endpoint

#### Syntax

radius override nas-ip-addr tunnel-client-endpoint

no radius override nas-ip-addr

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the RADIUS client (LNS) to override the standard use of the NAS-IP-Address [4] RADIUS attribute and instead use the tunnel-client-endpoint (LAC) IP address. The no version restores the default address.

#### Mode

Global Configuration