# Monitoring the Calling-Station-Id RADIUS Attribute

#### Purpose

Display the format and delimiter used for the Calling-Station-Id [31] attribute.

#### Action

To display the format configured for the Calling-Station-Id [31] attribute:

    host1#show radius calling-station-format
    fixed-format-adapter-new-field (includes SVLAN ID)

To display the delimiter used in the Calling-Station-Id for authenticated ATM PPP users:

    host1#show radius calling-station-delimiter
    &

#### Related Documentation

- show radius calling-station-format
- show radius calling-station-delimiter