# tunnel mpls autoroute announce

#### Syntax

[ no ] tunnel mpls [ traffic-eng ] autoroute announce [ ospf | isis ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the LSP tunnel to register its endpoint (the egress router) with the configured routing protocol so that the protocol can use the tunnel to determine routes. If you do not specify a routing protocol, the default is both IS-IS and OSPF. The no version disables endpoint announcements.

#### Options

- traffic-eng—Specifies optional keyword for compatibility with non–E Series implementations
- ospf—Endpoint is announced to OSPF
- isis—Endpoint is announced to IS-IS

#### Mode

Interface Configuration, Tunnel Profile Configuration