# subscriber-interface-type

#### Syntax

subscriber-interface-type subscriberInterfaceType

no subscriber-interface-type { subscriberInterfaceType | all }

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Assigns a subscriber-interface type to a QoS parameter definition. Subscriber-interface types represent subscriber interfaces to which QoS clients can apply QoS parameter instances obtained through RADIUS, SRC, or QoS profiles. You can specify up to four subscriber-interface types for each parameter definition. The no version removes the subscriber-interface type from the parameter definition.

#### Options

- subscriberInterfaceType—One of the following subscriber-interface types: atm-vc, ip, ipv6, l2tp-session, vlan
- all—Removes all subscriber-interface types

#### Mode

QoS Parameter Definition

#### Related Documentation

- Configuring a Basic Parameter Definition for QoS Administrators