Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- show ipv6 dhcpv6-local binding

# Monitoring DHCPv6 Local Server Binding Information

#### Purpose

Display the mapping between one or more IPv6 addresses and the DHCP unique ID of the subscriber’s computer.

#### Action

To display the DHCP binding information for an IPv6 address:

    host1#show ipv6 dhcpv6-local binding 2001:db8:4::/48

       Prefix           Client DUID        Lease            Intf
    -------------   -------------------   --------   ------------------
    2001:db8:4::/48 <LL 1/00A0DE113502>   infinite   FastEthernet 3/6.1

#### Meaning

Table 1 lists the show ipv6 dhcpv6-local binding command output fields.

Table 1: show ipv6 dhcpv6-local binding Output Fields

Field Name | Field Description
--- | ---
Prefix | IPv6 address
Client DUID | DHCP unique ID of subscriber’s computer
Lease | Time for which the IPv6 address is available in seconds, or infinite
Intf | Router’s interface that is associated with the subscriber’s computer

## Related Documentation

- show ipv6 dhcpv6-local binding

#### Published: 2010-10-12

Help
|
My Account
|
Log Out