Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- QoS for 802.3ad Link Aggregation Interfaces Overview
- Hashed Load Balancing for 802.3ad Link Aggregation Groups Overview
- interface lag
- node
- qos-profile
- queue

# Configuring the Scheduler Hierarchy for Hashed Load Balancing in 802.3ad Link Aggregation Groups

The type of load balancing that the system performs depends on the configuration of the scheduler hierarchy in the QoS profile.

To configure the scheduler hierarchy for hashed load balancing:

1. Configure a QoS profile.
   host1(config)#qos-profile hashed-lag
2. Configure the nodes and queues, including an Ethernet queue.
   host1(config-qos-profile)#ethernet queue traffic-class best-effort host1(config-qos-profile)#ethernet queue traffic-class tc1 host1(config-qos-profile)#ethernet queue traffic-class tc2
3. Create the LAG interface and attach the QoS profile.
   host1(config)#interface lag lg1 host1(config-if)#qos-profile hashed-lag

## Related Documentation

- QoS for 802.3ad Link Aggregation Interfaces Overview
- Hashed Load Balancing for 802.3ad Link Aggregation Groups Overview
- interface lag
- node
- qos-profile
- queue

#### Published: 2010-10-04

Help
|
My Account
|
Log Out