# Index

Symbols A B C D E F G H I J K L M N O P Q R S T U V W X

Symbols

> --More-- prompt 1, 2, 3, 4, 5
> .cnf files 1, 2, 3, 4, 5, 6, 7, 8, 9
> .dmp files 1, 2, 3, 4
> .hty files 1, 2, 3
> .log files 1, 2
> .pub files 1, 2, 3
> .rel files
>   specifying for reboot 1, 2
> .scr files 1, 2, 3
> .sts files 1, 2, 3
> .txt files 1, 2, 3
> 3des-cbc encryption algorithm for SSH 1, 2
> ? command 1, 2, 3

A

> AAA (authentication, authorization, accounting)
>   configuring
> aaa commands
>   aaa accounting vr-group
>   aaa authentication enable default
>   aaa authentication login 1, 2
>   aaa domain-map 1, 2
>   aaa local database
>   aaa local username
>   aaa new-model
>   aaa profile
> AAA Profile Configuration mode 1, 2
> AAL5 layer (ATM)
> abbreviating keywords
> abbreviations and acronyms
> access and uplink methods
> access levels (CLI)
> access lists
>   for Telnet sessions
> access-class in command
> access-list command 1, 2
> adapter commands
>   adapter accept
>   adapter disable
>   adapter enable
>   adapter erase
> Address Family Configuration mode 1, 2
> address-family ipv4 command
> address-family vpnv4 command
> agent, SNMP 1, 2
> algorithm negotiation, SSH
> arrow keys 1, 2, 3
> assembly numbers, displaying for hardware
> assembly revisions, displaying for hardware
> assigning an IP address 1, 2, 3, 4
> ATM interfaces
> ATM VC Class Configuration mode 1, 2
> ATM VC Configuration mode 1, 2
> attributes, SNMP
> authentication
>   AAA
>   FTP server
>   hmac-md5 for SSH
>   hmac-sha1 for SSH
>   hmac-sha1-96 for SSH
>   new model AAA
>   SSH user
> authentication trap, SNMP
> authorization
>   AAA
> Automatic Commit mode
> automatic synchronization
>   disabling
>   enabling
> autoupgrade
> avp command

B

> B-RAS applications
>   overview
> B-RAS commands
>   aaa accounting vr-group
> backing up software configuration
> Backspace key
> backup router
> bandwidth
>   associated error messages
>   line modules
>   SRP modules
> bandwidth errors
>   troubleshooting
> bandwidth oversubscription
>   configuring
>   monitoring
>   overview
> bandwidth oversubscription command
> banner command
> banners
>   configuring
> baseline commands
>   baseline show-delta-counts
>   baseline snmp
> BGP (Border Gateway Protocol)
> blowfish-cbc encryption algorithm for SSH
> boot commands
>   boot backup
>   boot config
>   boot config factory-defaults
>   boot config once
>   boot config running-configuration
>   boot config startup-configuration
>   boot force-backup
>   boot hotfix
>   boot revert-tolerance
>   boot revert-tolerance never
>   boot subsystem
>   boot system
> Boot mode
>   accessing
>   software installation
> booting the system
>   rebooting
>   while running scripts or macros
> Border Gateway Protocol., See BGP
> bottom-up approach to network configuration
> bridge commands
>   bridge subscriber-policy
> broadcasts, NTP
> bulk statistics, SNMP
>   collecting 1, 2
>   configuring
>     collectors and receivers
>     schemas
>   formatter
>   if-stats objects 1, 2, 3
>   mapping to MIBs and CLI
>   monitoring
>     collection statistics
>     schema statistics
> bulkstats commands, See also show bulkstats commands
>   bulkstats collector 1, 2, 3, 4
>   bulkstats collector collect-mode
>   bulkstats collector description
>   bulkstats collector interval
>   bulkstats collector max-size
>   bulkstats collector primary-receiver
>   bulkstats collector secondary-receiver
>   bulkstats collector single-interval
>   bulkstats file-format endOfLine-Lf
>   bulkstats interface-type
>   bulkstats interfaces description-format common
>   bulkstats receiver remote-name
>   bulkstats schema
>   bulkstats schema subtree
>   bulkstats schema subtree policy
>   bulkstats traps
>   bulkstats virtual-router-group

C

> caching, configuration
> capitalization., See case sensitivity
> case sensitivity
> channelized E1 interfaces
>   configuring
> channelized T1 interfaces
>   configuring
> channelized T3 interfaces
>   configuring
>   line rates
> characters on terminal screen, setting bits for 1, 2
> Classifier Group Configuration mode 1, 2
> clear commands
>   clear line
> CLI (command-line interface)
>   abbreviating keywords 1, 2
>   accessing
>   command modes., See command modes
>   context-sensitive help 1, 2
>   editing keys
>   editing on
>   logging in
>   pausing
>   system prompts
> CLI access levels, VSA descriptions 1, 2
> CLI command execution by macro file
> CLI messages
>   configuring
> CLI status indicator
> client, SNMP
>   configuring access 1, 2
> clock
> clock commands
>   clock set
>   clock summer-time date
>   clock summer-time recurring
>   clock timezone
> cOCx/STMx interfaces
>   line rates
> coldStart, SNMP trap
> Color Mark Profile Configuration mode 1, 2
> color-mark-profile command
> command history keys
> command modes
>   accessing
>   exiting 1, 2
> command-line interface., See CLI
> command-line prompts
> commands
>   abbreviating
>   editing on CLI
>   issuing from other command modes 1, 2, 3
>   listing available
>   pausing before executing
>   using
> commands for troubleshooting
> community table, SNMP
>   community name
>   configuring
>   IP access list
>   privilege levels
> community, SNMP 1, 2, 3
> configuration caching
> configuration file
>   running
> configuration modes., See command modes
> configuration tasks, general
> configuration, software 1, 2
> configure command 1, 2, 3
> configuring., See specific feature or protocol
> confirmations explicit command
> console
>   monitoring settings
>   password
>   restricting login
>   setting speed
> console lines
>   clearing
> contact person for SNMP server
> context-sensitive help 1, 2
> control flow monitoring
> Control Plane Configuration mode 1, 2, 3
> control plane security
> control-plane command
> controller commands
> Controller Configuration mode 1, 2
> conventions
>   notice icons
>   text and syntax
> copy commands
>   copy 1, 2, 3
>   copy running-configuration
>   copy running-configuration startup-configuration
>   copy startup-configuration
>   examples
> copying the software release file 1, 2, 3
> core dump files for troubleshooting 1, 2
> core dumps
> corrupted files., See flash cards, scanning
> crypto key dss command
> Ctrl-key combinations (CLI)
>   command history
>   command-line editing
> current configuration
>   saving 1, 2
> customer support
>   contacting JTAC
>   gathering information for

D

> data link-layer interfaces
>   configuring
> data set ready signal., See DSR
> data-character-bits command
> default version
> default virtual router
> delete command
> Delete key
> denial of service (DoS)
>   attaching groups
>   attacks
>   group parameters
>   protection
>   protocol mapping
> DHCP Pool Configuration mode 1, 2, 3
> diag command
> diag-level command
> diagnostics
>   enabling at warm restart
> Diffie-Hellman key exchange
> digital subscriber line access multiplexers., See DSLAMs
> dir command
> disable command 1, 2
> disable-autosync command
> disconnect ssh command
> display terminal
>   configuring
> displaying configuration information., See show commands
> distributed denial of service (DDoS) attack
> distribution lists
> DNS (Domain Name System)
>   configuring
> do command 1, 2, 3
> documentation set
>   comments on
> Domain Map Configuration mode 1, 2
> Domain Map Tunnel Configuration mode 1, 2
> DoS protection group commands
>   atm dos-protection-group
>   bridge1483 dos-protection-group
>   dos-protection-group
>   ethernet dos-protection-group
>   frame-relay dos-protection-group
>   hdlc dos-protection-group
>   ip dos-protection-group
>   ipv6 dos-protection-group
>   lag dos-protection-group
>   ppp dos-protection-group
>   pppoe dos-protection-group
>   priority burst
>   priority over-subscription-factor
>   priority rate
>   protocol burst
>   protocol drop-probability
>   protocol priority
>   protocol rate
>   protocol skip-priority-rate-limiter
>   protocol weight
>   use canned-group
>   vlan dos-protection-group
> Down Arrow key
> draft RFCs
> Drop Profile Configuration mode 1, 2
> drop-profile command
> DS1 channels
> DS3 channels
> DSLAMs (digital subscriber line access multiplexers) 1, 2, 3, 4
> DSR (data set ready), restricting login with
> dsr-detect command
> dump files, core

E

> E120 and E320 Broadband Services Routers
>   managing
> E3 interfaces
>   line rates
> E320 Broadband Services Routers
>   interface specifiers
> edge aggregation applications
>   private line aggregation
> editing on command-line interface
> enable commands
>   enable 1, 2, 3, 4
>   enable password
>   enable privilege-level
>   enable secret
> enable passwords, erasing
> encrypt passwords
> encryption
>   3des-cbc for SSH
>   blowfish-cbc for SSH
>   configuring SSH
>   twofish-cbc for SSH
> end command
> Enter key 1, 2, 3
> Enterprise SNMP MIB
> entity, SNMP
> environment, system
> erase secrets command 1, 2
> Esc-key combinations (CLI)
> Ethernet
>   Telnet on
> Ethernet port on SRP module
>   monitoring
> events
>   SNMP
> exception commands, See also show exception commands
>   exception dump
>   exception gateway
>   exception monitor
>   exception protocol ftp
>   exception source
> exclude-subsystem command
> exec-banner command
> exec-timeout command
> exit command 1, 2
> exiting the system
> Explicit Path Configuration mode 1, 2
> E Series routers
>   assigning IP address to
>   booting 1, 2, 3, 4
>   remote access., See B-RAS applications

F

> Fast Ethernet interfaces
>   specifying an interface
> file corruptions
> file system configuration, saving current
> files
>   copying 1, 2, 3
>   deleting
>   macro
>   managing
>   monitoring
>   redirecting
>   renaming
>   transferring
>   types of
>   viewing
> flash (NVS or nonvolatile storage) cards
>   copying
>   device names
>   different capacities
>   E120 and E320 Broadband Services Routers features
>   formatting
>   halt command to prevent corruption
>   installing
>   managing
>   monitoring
>   primary
>   rebooting and configuration data
>   rebooting in response to corrupt sectors
>   replacing
>   scanning
>     physical errors
>     structural errors in data
>   scanning utility
>   secondary
>   synchronizing
>   synchronizing with different capacities
>   validating and recovering file integrity
> flash-disk commands
>   flash-disk compare
>   flash-disk duplicate
>   flash-disk initialize
>   flash-disk scan
> Frame Relay interfaces
> FTP access
>   configuring
> FTP client
> FTP server
>   authentication
>   configuring
>   monitoring
> ftp-server enable command

G

> Get operation, SNMP
> GetBulk operation, SNMP
> GetBulk PDU type, SNMP
> GetNext operation, SNMP
> GetNextRequest PDU type, SNMP
> GetRequest PDU type, SNMP
> GetResponse PDU type, SNMP
> Global Configuration mode
>   exiting
> group, SNMP

H

> halt command 1, 2
> hardware
>   monitoring information
>   standards
>   versions, displaying 1, 2
> HDLC parameters
> help
>   CLI system
> help command 1, 2, 3
> history command
> hmac-md5 authentication for SSH
> hmac-sha1 authentication for SSH
> hmac-sha1-96 authentication for SSH
> host command
> host ftp command
> host table, modifying 1, 2
> hostname command
> hotfix activate command
> hotfix files, monitoring
> hotfixes
>   activating
>   arming
>   backup settings and
>   compatibility
>   dependencies
>   displaying
>   hot-patchable
>   startup
>   synchronizing on SRP modules

I

> I/O adapters., See IOAs
> I/O modules
>   software compatibility
> if constructs, macro
> ILMI (integrated local management interface)
> image on primary SRP module, copying
> installing system software
>   required information 1, 2, 3
> interactive help system., See help
> interface commands
>   interface 1, 2, 3
>   interface fastEthernet
>   interface loopback
> Interface Configuration mode 1, 2
> interfaces
>   configuring
>   Fast Ethernet
>   physical, configuring 1, 2
>   shared interfaces
>   subscriber interfaces
> IOA configurations
>   deleting 1, 2
> IOAs
>   disabling 1, 2
>   enabling
>   erasing configurations 1, 2
>   replacing
> IP access list, SNMP
> IP addresses
>   assigning 1, 2, 3
>   configuring
> ip commands
>   ip atm-vc
>   ip dhcp-local pool
>   ip domain-lookup 1, 2
>   ip domain-lookup transit-virtual-router
>   ip domain-name
>   ip ftp source-address
>   ip ftp source-interface
>   ip name-server
>   ip vrf 1, 2
> IP multicast
> IP NAT Pool Configuration mode 1, 2
> ip nfs commands
>   ip nfs
>   ip nfs host
> ip rate-limit-profile command
> ip ssh commands
>   ip ssh authentication-retries
>   ip ssh crypto
>   ip ssh disable-user-authentication
>   ip ssh mac
>   ip ssh sleep
>   ip ssh timeout 1, 2
> IP support
>   IP/ATM
>   IP/Ethernet
>   IP/FR
>   IP/HDLC
>   IP/PPP
> IP tunnels
> ip vrf commands
>   ip vrf
> IPSec (IP Security)
>   AH
>   ESP
> IPSec CA Identity Configuration mode
> ipsec commands
>   ipsec ca identity
>   ipsec identity
>   ipsec ike-policy-rule
>   ipsec key manual
>   ipsec key pubkey-chain rsa
> IPSec Identity Configuration mode 1, 2
> IPSec IKE Policy Configuration mode 1, 2
> IPSec Manual Key Configuration mode 1, 2, 3
> IPSec Peer Public Key Configuration mode 1, 2
> IPSec Transport Profile Configuration mode 1, 2
> IPSec Tunnel Profile Configuration mode
> IPv6 Local Configuration mode
> IPv6 Local Pool Configuration mode
> IS-IS protocol
> issuing commands from other CLI modes 1, 2, 3

J

> Juniper Networks E Series enterprise SNMP MIB

K

> keywords
>   partial-keyword

L

> L2 Transport Load-Balancing-Circuit Configuration mode 1, 2
> L2C commands
>   l2c
>   neighbor
> L2TP (Layer 2 Tunneling Protocol)
> l2tp commands
>   l2tp destination profile
>   l2tp rate-limit-profile
>   l2tp switch-profile
> L2TP Destination Profile Configuration mode 1, 2
> L2TP Destination Profile Host Configuration mode 1, 2
> L2TP Tunnel Switch Profile Configuration mode 1, 2
> Layer 2 Control Configuration mode 1, 2
> Layer 2 Control Neighbor Configuration mode 1, 2
> Layer 2 Tunneling Protocol., See L2TP
> layered approach to network configuration
> LDP Configuration mode 1, 2
> Left Arrow key
> levels of CLI access
> line command 1, 2, 3
> Line Configuration mode 1, 2
> line module configurations
>   deleting 1, 2
> line modules
>   allowed combinations 1, 2
>   bandwidth
>   combinations 1, 2
>   disabling 1, 2
>   enabling
>   erasing configurations 1, 2, 3
>   initialization sequence
>   line rates
>   performance rate
>   replacing
>   restricted combinations
>   slot groups 1, 2, 3
>   software
>     compatibility
>   switch usage
>   troubleshooting
> line rates
> line vty command 1, 2
> lines
>   clearing
>   configuring
>   monitoring
>   setting on terminal screen
> link-up, link-down traps, SNMP
> linking to an FTP server., See FTP access
> listing commands available
> listing configuration settings., See show commands
> listing files on system
> LMI (local management interface) 1, 2, 3
> Local IPSec Transport Profile Configuration mode 1, 2, 3
> Local User Configuration mode 1, 2, 3
> location of SNMP server
> log commands
>   log severity
> logging in to system
> logging system events
>   viewing logs
> login banner
> login commands
>   login 1, 2, 3
>   login authentication
> login conditions
>   configuring
> long scripts, copying

M

> MAC (media access control) addresses
>   configuring for SSH
> macro (.mac) files 1, 2
> macro command
> macros
>   comments
>   conditional execution
>   control expressions
>   environment commands
>   if constructs
>   invoking from another macro file 1, 2
>   literals
>   naming
>   noncontrol expressions
>   operators
>     arithmetic
>     assignment
>     extraction
>     increment and decrement
>     logical
>     miscellaneous
>     relational
>     string
>   resetting system while running
>   variables
>   while constructs
>   writing 1, 2
> managed object, SNMP
> Management Information Bases., See MIBs
> Manual Commit mode
> manuals
>   comments on
> Map Class Configuration mode 1, 2
> Map List Configuration mode 1, 2
> map-class frame-relay command
> map-list command
> master router
> master, NTP
> MD5 authentication
>   SSH
> memory (hardware), displaying
> memory management
> memory warning command
> message authentication code., See MAC addresses
> message-of-the-day (MOTD) banner 1, 2
> MIBs (Management Information Bases)
>   definition of
>   Juniper Networks E Series enterprise
>   standard SNMP
> modules
>   disabling
>   E Series, managing
>   E120 and E320 Broadband Services Routers
>   enabling
>   monitoring
>   replacing
> monitor., See terminal
> more command
> motd-banner command
> mount command
> mounting a CD on an FTP server 1, 2, 3
> MPLS (Multiprotocol Label Switching)
> mpls commands
>   mpls explicit-path name
>   mpls ldp profile
>   mpls rsvp profile
>   mpls tunnels profile
> Multiprotocol Label Switching., See MPLS

N

> names
>   renaming local files
>   system name
> network configuration
>   layered (bottom-up) approach
>   routing protocols
> network elements, SNMP
> Network File System., See NFS client
> network planning
>   access lists
>   BGP
>   COCX-F3 modules
>   configurable HDLC parameters
>   configuration overview 1, 2
>   CT3 12-F0 modules
>   data link-layer interfaces
>   distribution lists
>   E3 modules
>   Ethernet modules
>   general configuration tasks
>   interfaces and subinterfaces
>   IP multicast
>   IP/ATM
>   IP/Frame Relay
>   IP/HDLC
>   IP/PPP
>   L2TP
>   layered approach
>   line module features
>   MPLS
>   non-PPP equal access
>   OSPF 1, 2
>   physical layer interfaces
>   policy management
>     configuring
>   private line aggregation
>   RIP
>   route maps
>   routing policy
>   routing protocols
>   SONET
>   virtual routers
>   VRRP
> network servers, displaying list of
> Network Time Protocol., See NTP
> new model AAA authentication
> NFS client
>   configuring
>   overview
> no boot hotfix all-releases command
> no command 1, 2
> non-PPP equal access
> nonvolatile storage., See flash (NVS or nonvolatile storage) cards
> notice icons
> NTP (Network Time Protocol)
>   best server
>   broadcasts
>   client-server associations
>   configuring
>   master
>   monitoring 1, 2
>   overview
>   peers
>   replies
>   requests
>   servers 1, 2, 3
>   synchronization
>   virtual routers 1, 2
> NTP client
>   configuring the system as
>   system operation as
> ntp commands, See also show ntp commands
>   ntp access-group
>   ntp broadcast
>   ntp broadcast-client
>   ntp broadcast-delay
>   ntp disable
>   ntp enable
>   ntp master
>   ntp server
>   ntp server enable
>   ntp source
> NTP control queries
> NTP servers
>   assigning
>   best
>   choosing
>   configuring virtual routers as
>   enabling NTP broadcasting
>   enabling on a virtual router
>   primary
>   selecting
>   system operation as

O

> objects, tracking reachability 1, 2, 3
> OC48/STM16 interfaces, configuring
> OCx/STMx interfaces
>   configuring
> Open Shortest Path First., See OSPF
> OSPF (Open Shortest Path First)
> output filtering
>   from the --More-- prompt
>   show command
> oversubscription, bandwidth
>   configuring
>   monitoring
>   overview
> overview, NTP

P

> packet mirroring
>   and SNMP
> packet size, SNMP
> pagination keys
> parameters 1, 2
> parent-group command 1, 2, 3
> partial releases, copying
> password command 1, 2, 3, 4
> passwords, See also Privileged Exec mode
>   enabling
>   encryption
>   erasing console passwords
> passwords and secrets
>   deleting
> patching the system with hotfixes
> pausing before command execution
> PDU (protocol data unit)
> performance rate, line modules
>   configuring
> physical errors in flash cards
> physical interfaces, configuring 1, 2
> physical slots
>   rebooting selected
> ping command 1, 2
> platform considerations
>   installing JunosE Software
>   macros
>   managing modules
>   network planning
>   passwords and security
>   SNMP
>   system booting
>   system clock
>   system management
>   using the CLI
>   virtual routers
> Policy List Configuration mode 1, 2
> Policy List Parent Group Configuration mode 1, 2, 3, 4, 5, 6, 7, 8, 9
> policy management
>   QoS classification and marking
>   rate limiting
>   types of services 1, 2
>   xDSL session termination
> polling NTP servers
> POS interfaces
> PPP (Point-to-Point Protocol)
>   protocol support
> PPPoE Service Name Table Configuration mode 1, 2
> pppoe-service-name-table command
> primary flash card
>   initializing
>   reformatting
> primary NTP servers
> private line aggregation
> privilege groups
> privilege level
>   accessing
>   ambiguous commands
>   changing command privileges
>   command exceptions
>   defining CLI
>   keyword mapping
>   password encryption
>   setting
>     default line
>     multiple commands
>     no or default versions
>   SNMP
>   viewing information
> privilege level command
> Privileged Exec mode, See also passwords
>   accessing 1, 2, 3, 4, 5, 6
>   exiting 1, 2, 3
> privileged-level access (CLI) 1, 2, 3, See also Privileged Exec mode
> profile commands
>   profile
> Profile Configuration mode 1, 2
> progress indicator (CLI)
> prompts, CLI system
> protocol data unit., See PDU
> proxy, SNMP 1, 2
> pvc command

Q

> QoS (quality of service)
> QoS commands
>   qos-profile command
> QoS Interface Set Configuration mode 1, 2
> QoS Interface Superset Configuration mode 1, 2
> QoS Parameter Configuration mode
> QoS Parameter Definition Configuration mode 1, 2
> QoS Profile Configuration mode 1, 2
> QoS Shared Shaper Control Configuration mode
> qos-profile command
> qos-shared-shaper-control command
> Queue Profile Configuration mode 1, 2
> queue-profile command

R

> RADIUS (Remote Authentication Dial-In User Service)
>   authentication, restricting access
>   password authentication
>   per-user enable authentication
>   restricting access to commands 1, 2
>   user authentication
> radius commands
>   radius accounting server
>   radius authentication server
>   radius dynamic-request server
> RADIUS Configuration mode 1, 2
> radius relay commands
>   radius relay accounting server
>   radius relay authentication server
> RADIUS Relay Configuration mode
> Rate Limit Profile Configuration mode 1, 2
> rate limiting
>   per priority
>   per protocol
> reachability, tracking
> reaching an FTP server., See FTP access
> reboot history (reboot.hty) file
> reboot history, displaying
> rebooting the system
> redistribute routes
> Redundancy Configuration mode 1, 2
> references
>   draft RFCs
>   hardware standards
>   non-RFC software standards
>   RFCs
> refusing NTP broadcasts
> regular expressions
>   metacharacters
>     specifying as literals
> releasing available memory
> reload commands
>   reload 1, 2
>   reload at
>   reload in
>   reload slot
> Remote Authentication Dial-In User Service., See RADIUS
> remote host command
> Remote Neighbor Configuration mode 1, 2
> remote-neighbor command
> rename command
> renaming files
> replies, NTP
> reset button, software
> resetting while running scripts or macros
> resource commands
>   resource if-type
>   resource threshold
> resources
>   monitoring
> revisions, displaying assembly
> RFC 1213 interface numbering
> RFCs
>   draft
> Right Arrow key
> RIP (Routing Information Protocol)
> Route Map Configuration mode 1, 2
> route maps
> route-map command
> router commands
>   router
>   router bgp
>   router ospf
>   router pim
>   router rip 1, 2
> Router Configuration mode 1, 2
> routers., See system
> Routing Information Protocol., See RIP
> routing policy
>   configuring
> routing protocols
>   configuring
> routing, IP
>   configuring other protocols
>   monitoring
> RSVP Configuration mode 1, 2
> rtr commands
>   rtr
> RTR Configuration mode 1, 2
> run command 1, 2, 3

S

> schedule-profile command
> Scheduler Profile Configuration mode 1, 2
> screen., See terminal
> script files
> scripts
>   resetting system while running
> secondary NTP servers
> secure IP tunnels
> Secure Shell Server protocol., See SSH
> security
>   administration through SSH instead of Telnet
>   SSH issues
> security features of SNMP
> send command
> sending messages to terminals
> serial numbers, displaying for hardware
> servers, NTP
> service commands
>   service
>   service ctrl-x-reboot 1, 2
>   service manual-commit
>   service password-encryption 1, 2
>   service unattended password-recovery
> Service Manager commands
>   service-management service-session-profile
> Service Session Profile Configuration mode 1, 2
> Set operation, SNMP
> SetRequest PDU type, SNMP
> SFMs (switch fabric modules)
>   accepting configurations
>   disabling 1, 2
>   enabling
>   erasing configurations
>   overview
>   replacing
> shared interfaces
> show aaa commands
>   show aaa domain-map
> show bandwidth oversubscription
> show boot command
> show bulkstats commands
>   show bulkstats
>   show bulkstats collector interface-type
>   show bulkstats collector interval
>   show bulkstats collector max-size
>   show bulkstats collector transfer-mode
>   show bulkstats receiver
>   show bulkstats router-group
>   show bulkstats statistics
>   show bulkstats traps
> show command output, filtering
> show commands
>   show output filtering feature 1, 2
>   show policy-list
>   show redirecting output
> show configuration commands
>   show configuration 1, 2
>   show configuration category
>   show configuration interface
>   show configuration virtual-router 1, 2
> show dos-protection-group
> show environment command
> show exception commands
>   show exception dump
>   show exception monitor
> show fabric weights command
> show flash command
> show ftp-server command
> show hardware command 1, 2
> show hosts command
> show hotfix command
> show ip commands
>   show ip domain-lookup command
>   show ip forwarding-table slot
>   show ip ssh
> show ip nfs command
> show last-reset command
> show line console 0 command
> show line vty command 1, 2
> show log commands
>   show log data
> show memory-management protection command
> show ntp commands
>   show ntp associations
>   show ntp associations detail
>   show ntp status
> show nvs command
> show processes command 1, 2
> show reboot-history command
> show reload command
> show running-configuration command 1, 2
> show secrets command
> show snmp commands
>   show snmp
>   show snmp community
>   show snmp interfaces
>   show snmp notificationLog
>   show snmp trap
>   show snmp trapstat
> show subsystems command
> show suspicious-control-flow-detection commands
>   show suspicious-control-flow-detection counts
>   show suspicious-control-flow-detection flows
>   show suspicious-control-flow-detection info
>   show suspicious-control-flow-detection protocol
> show tech-support command
> show terminal command 1, 2
> show timing command
> show users command
> show utilization command 1, 2
> show version command 1, 2, 3, 4
> show virtual-router command
> Simple Network Management Protocol., See SNMP
> sleep command
> slot commands
>   slot accept
>   slot disable
>   slot enable
>   slot erase 1, 2
> slot groups and module arrangements 1, 2
> SNMP (Simple Network Management Protocol)
>   agent software 1, 2
>   attributes
>   bulk statistics collection
>   client software
>     configuring access 1, 2
>   communities 1, 2, 3
>   compressing interfaces
>   configuration tasks
>   enabling
>   encoding method
>   engine
>   entity
>   group
>   interface numbering
>   management features
>   managing interface sublayers
>   memory warning
>   monitoring interface tables
>   monitoring status 1, 2
>   multiple virtual routers 1, 2
>   operations
>   packet mirroring
>   packet size, setting
>   PDU
>   proxy, creating
>   RFC 1213 compatibility
>   schema
>     configuring
>     monitoring
>   security features
>   server
>   server parameters, setting
>   traps., See SNMP traps
>   users, configuring
>   versions
>   view 1, 2
>   viewing status
>   virtual routers
> SNMP commands, See also bulkstats commands
>   agent context-name
>   bulkstats interfaces rfc 1213
>   delta-sampling
>   enable
>   event
>   frequency
>   notification id
>   resource
>   trigger
> snmp commands
>   snmp interfaces description-format
>   snmp trap ip link-status
>   snmp trap link-status
>   snmp-server
>   snmp-server community
>   snmp-server contact
>   snmp-server enable traps
>   snmp-server host 1, 2, 3
>   snmp-server interfaces compress
>   snmp-server interfaces compress-restriction
>   snmp-server interfaces rfc1213
>   snmp-server location
>   snmp-server notificationLog ageOut
>   snmp-server notificationLog entryLimit
>   snmp-server notificationLog log
>   snmp-server packetsize
>   snmp-server trap-proxy
>   snmp-server trap-source
>   snmp-server user
> SNMP Event Manager Configuration mode 1, 2
> SNMP traps
>   enabling
> software
>   compatibility
>   configuration
>     backing up
>     saving
>   installing 1, 2
>   line rates
>   release file
>   updating
>   upgrading 1, 2, 3
> software release file
>   accessing 1, 2, 3
>   specifying for reboot
> software reset button
> software standards
>   draft RFCs
>   non-RFC standards
>   RFCs
> software versions, displaying 1, 2
> Space key 1, 2
> speed command
> SRP module configurations
>   deleting 1, 2
> SRP module redundancy
>   hotfixes and
>   validating and recovering file integrity
> SRP modules
>   bandwidth
>   configuring
>   copying image
>   core dump file
>   disabling
>   enabling
>   erasing configurations 1, 2
>   overview
>   removing
>   replacing
>   reset button
>   synchronizing
> SSH (Secure Shell Server)
>   algorithm negotiation
>   client configuration
>   configuration prerequisites
>   configuring
>   connections
>   disabling
>   enabling
>   encryption algorithms
>     3des-cbc
>     blowfish-cbc
>     twofish-cbc
>   encryption, configuring
>   generating host keys
>   host key management
>   key exchange
>   message authentication
>     configuring
>     hmac-md5
>     hmac-sha1
>     hmac-sha1-96
>   monitoring
>   performance issues
>   security concerns
>   server public key files
>   terminating
>   user authentication
>     configuring
>   user key management
> standards
>   draft RFCs
>   hardware standards
>   non-RFC software standards
>   RFCs
> startup configuration
>   saving
> static host maps, adding 1, 2
> static tunnels
> statistics
>   SNMP 1, 2
> statistics (.sts) files
> Statistics Profile Configuration mode 1, 2
> statistics-profile command
> status indicator (CLI)
> stratum 1 servers., See NTP servers, primary
> structural errors in flash data
> Subinterface Configuration mode 1, 2
> subinterfaces
>   configuring
> subscriber interfaces
> subscriber policy commands
>   subscriber-policy
> Subscriber Policy Configuration mode 1, 2
> summer time, specifying
> support, technical, See technical support
> suspicious control flow detection
>   display options
>   logs
>   parameters
>   traps
> suspicious control flow monitoring
> suspicious-control-flow-detection commands
>   baseline suspicious-control-flow-detection counts
>   clear suspicious-control-flow-detection
>   suspicious-control-flow-detection grouping-off
>   suspicious-control-flow-detection off
>   suspicious-control-flow-detection protocol backoff-time
>   suspicious-control-flow-detection protocol low-threshold
>   suspicious-control-flow-detection protocol threshold
> switch fabric modules., See SFMs
> switch usage, line modules
> synchronization process 1, 2
> synchronization reserve file
> synchronize command 1, 2
> system
>   autoupgrade feature
>   basic parameters
>   booting
>     rebooting
>   command-line interface., See CLI
>   configuring automatically
>   environment information
>   exiting
>   FTP client
>   FTP server
>   initializing line modules
>   levels of access 1, 2
>   logging in
>   logging/troubleshooting, commands for 1, 2
>   managing
>   monitoring
>   passwords
>   patching with hotfixes
>   physical slots, rebooting
>   RADIUS password authentication
>   software reset button
>   system configuration files 1, 2
>   system name
>   TFTP client
>   timing
>   updating with hotfixes
>   virtual router limitations
> system clock
>   setting
> system commands
>   privilege
>   privilege-group alias
>   privilege-group membership
>   privilege-group membership clear
>   write core
> system configuration
>   saving current 1, 2, 3
>   saving startup
> system passwords., See passwords
> system security
> system.log file

T

> T1 lines, controllers for
> T3 interfaces
>   configuring
>   controllers for
>   line rates
> Tab key 1, 2, 3
> TACACS+
>   aaa authentication login
>   restricting access to commands
> tag-group command
> tech-support encoded-string command
> technical support
>   contacting JTAC
> Telnet
>   access lists
>   client, using
>   configuring to listen in nondefault virtual router
>   logins
> telnet commands
>   telnet
>   telnet listen
> terminal
>   configuring display
>   displaying configuration
>   displaying international characters 1, 2
>   sending messages to
>   setting length (in lines)
>   setting width (in characters)
> terminal commands, See also show terminal command
>   terminal data-character-bits
>   terminal length
>   terminal speed
>   terminal width
> text and syntax conventions
> text files
> TFTP client
> thermal protection mode
> time limits, setting
>   for user input
>   for user login
> time zone, specifying
> timeout login response command
> timing commands
>   timing disable-auto-upgrade
>   timing select
>   timing source
> timing, system, See also system clock
>   configuring
>   monitoring
> trace command
> tracking objects 1, 2, 3
> Traffic Class Configuration mode 1, 2
> Traffic Class Group Configuration mode 1, 2
> traffic-class command
> traffic-class-group command
> transport protocols, xDSL
> traps command
> traps, SNMP
>   categories
>   configuring
>   configuring notification logs for
>   configuring trap queues
>   operation
>   PDU type
>   recovering lost traps
>   severity levels
>   specifying an egress point for
>   statistics
>   status information
> troubleshooting core dump files
> tunnel commands
>   tunnel 1, 2
> Tunnel Group Configuration mode 1, 2, 3
> Tunnel Group Tunnel Configuration mode 1, 2, 3
> Tunnel Profile Configuration mode 1, 2
> Tunnel Server Configuration mode 1, 2
> tunnel-server command
> tunnels, IP
> twofish-cbc encryption algorithm for SSH

U

> Universal Coordinated Time., See UTC
> Up Arrow key
> updating the system software
> updating the system with hotfixes
> upgrading software
>   systems with one SRP module
>   systems with two SRP modules
> uplink methods
> user access, restricting
> user authentication, configuring 1, 2, See also authentication
> User Exec mode 1, 2, 3, See also Privileged Exec mode
> user interface commands
> user interface, customizing
> user level access (CLI)
> UTC (Universal Coordinated Time) 1, 2

V

> vc-class atm command
> vendor-specific attributes., See VSAs
> versions
>   default
>   displaying for hardware
>   displaying for hardware/software
>   displaying for software
>   SNMP
> view, SNMP 1, 2
> viewing files 1, 2, See also show commands
> virtual interfaces (subinterfaces)
> virtual router commands
>   ip vrf
>   virtual-router 1, 2, 3, 4
> Virtual Router Redundancy Protocol (VRRP)., See VRRP
> virtual routers
>   configuring 1, 2
>   default virtual router
>   map VR to domain map 1, 2
>   monitoring 1, 2
>   name resolvers for multiple
>   NTP 1, 2, 3, 4
>   restricting access
>   SNMP
>     managing
>   VPNs
>   VRFs
>   VSAs
>   with routing protocols 1, 2, 3
> VPN routing and forwarding instance., See VRF
> VPNs (virtual private networks)
> VR Group Configuration mode 1, 2
> VRF (VPN routing and forwarding instance)
> VRF Configuration mode 1, 2
> VRRP (Virtual Router Redundancy Protocol) 1, 2
> VSAs (vendor-specific attributes)
>   levels of CLI access
>   restricting access to virtual routers
> vty lines
>   clearing
>   configuring
>   managing
>   monitoring
>   users of

W

> waiting before command execution
> warm restart
>   enabling diagnostics at
> warmStart, SNMP trap
> while constructs, macro
> width of terminal screen, setting
> write memory command
> writing macros

X

> xDSL
>   protocols
>   session termination